**Change and repair log**

Any change in headset (except changing electrodes positions) **must be first approved by Or** ([orabani@campus.haifa.ac.il](mailto:orabani@campus.haifa.ac.il)).

**System #54**

|  |  |  |  |
| --- | --- | --- | --- |
| **date** | **change** | **done by** | **parts used** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

## Current electrode positions and wiring

|  |  |  |  |
| --- | --- | --- | --- |
| **GUI ID** | **10-20 Location** | **Wire Color** | **Pin ID** |
| -- | Ear Clip  Reference | Black, with white splitter | Cyton Bottom SRB pin (SRB2) |
| 1 | C3 | gray | Cyton Bottom N1P pin |
| 2 | C4 | blue | Cyton Bottom N2P pin |
| 3 | CP1 | green | Cyton Bottom N4P pin |
| **4** | **CP2** | **white** | **Cyton Bottom N3P pin** |
| 5 | FC1 | blue | Cyton Bottom N6P pin |
| 6 | FC2 | black | Cyton Bottom N5P pin |
| 7 | CP5 | white | Cyton Bottom N8P pin |
| 8 | CP6 | green | Cyton Bottom N7P pin |
| -- | Ear Clip -  Digital Ground and noise cancelling | Black | Cyton Bottom BIAS pin |
| -- | Ear Clip -  Reference | Black, with white splitter | Daisy Bottom SRB pin (SRB2) |
| 9 | FC5 | gray | Daisy Bottom N1P pin |
| 10 | FC6 | gray | Daisy Bottom N2P pin |
| 11 | T3 | black | Daisy Bottom N3P pin |
| 12 | T4 | purple | Daisy Bottom N4P pin |
| 13 | CZ | purple | Daisy Bottom N5P pin |
| 14 | ------- |  |  |
| 15 | ------- |  |  |
| 16 | ------- |  |  |

## 